Configuring PTZ Tracking via FreeD protocol for Panasonic AW-UE100 camera:

 - add video from the camera to a slot and enable PTZ control

 - load the scene into another slot and assign the video from the camera to the **overlay** texture

 - a parameter should appear in the texture properties - enable / disable Tracker

 - if Tracker is enabled, then tracking settings appear

 - Tracker Port - port number to which the camera sends PTZ coordinates, by default the port is the same as VISCA = 52381

 - Tracker Offset - the angle by which the virtual camera will be rotated relative to the real camera

 - Tracker Parallax - shift the axis of rotation of the virtual camera to compensate for the parallax that occurs due to the fact that in a real camera the optical axis does not coincide with the axis of rotation

 - Tracker Delay - delay PTZ coordinates for synchronization with video

 - Tracker Calibration - allows you to download the FOV-ZOOM calibration file

 - Tracker Calibration Calibrate icon - by pressing the calibration settings dialog appears

 - Tracker Calibration Reset icon - by pressing the default calibration curve is generated

 - calibration dialog - points on the graph can be edited by drag-drop

 - calibration dialog - if you click on any point, then the ptz camera starts sending commands to control the zoom speed, until the desired zoom value comes from the camera

 - calibration dialog - there is a highlighted sliding point on the chart showing the current state of the camera

 - calibration dialog - the graph is saved when the project is saved

 - demo project "\!ECGSoft\!AllMixProjects\AllMix\_Demo\_Projects\Tracking\"